**AC Corrosion and the Pourbaix Diagram**

Andreas Junker, M.Sc., Eng.
MetriCorr, Toerringvej 7, 2610 Roedovre Denmark
Technical University of Denmark, Produktionstorvet B425, 2800 Kgs. Lyngby, Denmark

Lars Vendelbo Nielsen, Ph.D., Eng.
MetriCorr, Toerringvej 7, 2610 Roedovre Denmark

Per Møller, Prof., Eng.
Technical University of Denmark, Nils Koppels Allé B404, 2800 Kgs. Lyngby, Denmark

**Abstract**

AC interference on cathodically protected pipelines is of major concern due to the risk of AC corrosion. Corrosion is generally linked to AC and DC current densities, but incoherence in data from different researches is often difficult to explain. In this paper, ER-probe corrosion rate data from multiple experiments will be used to illustrate how the accepted AC and DC current density criteria may in fact be closely linked to thermodynamically calculated Pourbaix diagrams. The concepts will be illustrated by simple model experiments and discussed in a theoretical context based on literature.

